1.PERFORM ACTIVE TEST (E-SUS CONTROL UNIT) With CONSULT-III

1. Connect the E-SUS control unit harness connector and rear RH shock absorber actuator harness connector.
2. Select “SHOCK ABSORBER ACTUATOR” in “ACTIVE TEST”.
3. On the display, change the “Operation half cycle”, and check that the operation noise is heard from the actuator.

   Test item | Display Item | Display
   Operation half cycle
   SHOCK ABSORBER ACTUATOR | REAR RIGHT ACTUATOR | 0.1 seconds – 1 second (cycle in 0.1 seconds)

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace the rear RH shock absorber. Refer to Removal and Installation (GT-R certified NISSAN dealer).