- The accelerator pedal position sensor is installed on the upper section of the accelerator pedal assembly and detects the depressing amount of the accelerator pedal. The accelerator pedal position sensor converts the depressing amount of the accelerator pedal into voltage signal and transmits it to ECM. ECM transmits the signal to TCM via the CAN communication.
- TCM selects the driving gear using the gear shift line and corrects the operation of the clutches and clutch actuators based on the signal.