DTC DETECTION LOGIC

DTC | Self-diagnosis name | DTC detection condition | Possible cause
P2776 | Upshift switch circuit low | A DTC is set if TCM detects the paddle shifter (shift-up switch) ON signal for a certain period of time. |

- Paddle shifter (shift-up switch)
- Harness or connector
  [Short in the paddle shifter (shift-up switch) circuit]

DTC CONFIRMATION PROCEDURE
1.PREPARATION BEFORE OPERATION
If another “DTC CONFIRMATION PROCEDURE” is performed just before the next test, turn the ignition switch OFF and wait for 10 seconds or more, then perform the next test.
>>GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDURE
With CONSULT-III

1. Start the engine and wait for 1 minute or more.
2. Check “Self Diagnostic Result” of “TRANSMISSION”.

Is DTC P2776 detected?
YES>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>Go to Intermittent Incident.