APPLICATION ITEM CONSULT-III performs the following functions via CAN communication with BCM.

Diagnosis mode | Function Description
DATA MONITOR | The BCM input/output signals are displayed.
ACTIVE TEST | The signals used to activate each device are forcibly supplied from BCM.

DATA MONITOR

Monitor item | Content
CONFRM ID ALL | Indicates [YET] at all time. Switches to [DONE] when a registered Intelligent Key is inserted into the key slot.
CONFIRM ID4
CONFIRM ID3
CONFIRM ID2
CONFIRM ID1
TP 4 | Indicates the number of ID which has been registered.
TP 3
TP 2
TP 1
PUSH SW | Indicates [ON/OFF] condition of push-button ignition switch.
KEY SW -SLOT | Indicates [ON/OFF] condition of key slot.

ACTIVE TEST

Test item | Description
THEFT IND | This test is able to check security indicator lamp operation. The lamp will be turned on when “ON” on CONSULT-III screen touched.