DTC DETECTION LOGIC

DTC | Display item | Malfunction detected condition | Possible cause
C1110 | CONTROLLER FAILURE | When there is an internal malfunction in the ABS actuator and electric unit (control unit). | ABS actuator and electric unit (control unit)

DTC CONFIRMATION PROCEDURE
1.DTC REPRODUCTION PROCEDURE

1. Turn the ignition switch ON.
2. Perform self-diagnosis for “ABS” with CONSULT-III.

Is DTC “C1110” detected?
YES>>Proceed to diagnosis procedure. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END