1.CHECK FUEL LEVEL SENSOR UNIT (MAIN) Check the resistance value of fuel level sensor unit (main).

2 – 3 |
Full | :Approx. 3.0 Ω
Empty | :Approx. 90.0 Ω

Standard float position

Full (A) [mm (in)] | :Approx. 282.2 (11.11)
Empty (B) [mm (in)] | :Approx. 19.2 (0.756)

Is the inspection result normal?
YES>>GO TO 2.
NO>>Replace the fuel level sensor unit (main).
2.CHECK FUEL LEVEL SENSOR UNIT (SUB)
Check the resistance value of fuel level sensor unit (sub).

1 – 2 |
Full | :Approx. 3.0 Ω
Empty | :Approx. 45.9 Ω

Standard float position

Full (A) [mm (in)] | :Approx. 29.9 (1.177)
Empty (B) [mm (in)] | :Approx. 218.3 (8.59)

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace the fuel level sensor unit (sub).