■ CAUTION ■

- Operate with two workers, because of its heavy weight.
- Support door with a jack and use protective tape or shop cloth to protect from damage during removal and installation.

REMOVAL

1.Disconnect the door harness connector.

2.Remove the door check link mounting bolts (body side).

3.Remove the door hinge mounting nuts (door side), and then remove the door assembly.

INSTALLATION
Install in the reverse order of removal.
■ CAUTION ■

- Never reuse bolts and nuts connecting the door hinge with the door striker. Use the specified bolts and nuts when installing.
- Apply anticorrosive agent onto the mounting surface.
- After installation, perform the fitting adjustment. Refer to Adjustment.
- After installation, apply touch-up paint (the body color) onto the head of door hinge mounting bolts and nuts.