Type |  | M000T22771
MITSUBISHII make
Reduction gear type
System voltage | [V] | 12
No-load | Terminal voltage | [V] | 11
Current | [A] | Less than 90
Revolution | [rpm] | More than 2,400
Minimum diameter of commutator | [mm (in)] | 28.8 (1.134)
Minimum length of brush | [mm (in)] | 5.5 (0.217)
Brush spring tension | [N (kg, lb)] | 15.0 – 20.5 (1.5 – 3.4, 2.1 – 4.6)
Clearance between bearing metal and armature shaft | [mm (in)] | Less than 0.2 (0.008)
Clearance between pinion front edge and pinion stopper | [mm (in)] | 0.5 – 2.0 (0.02 – 0.079)