DTC DETECTION LOGIC NOTE： If DTC P0442 is displayed with DTC P0456, first perform the trouble diagnosis for DTC P0456. Refer to DTC Logic (GT-R certified NISSAN dealer). This diagnosis detects leaks in the EVAP purge line using engine intake manifold vacuum.
If pressure does not increase, the ECM will check for leaks in the line between the fuel tank and EVAP canister purge volume control solenoid valve, under the following “Vacuum test” conditions.
The EVAP canister vent control valve is closed to shut the EVAP purge line off. The EVAP canister purge volume control solenoid valve will then be opened to depressurize the EVAP purge line using intake manifold vacuum. After this occurs, the EVAP canister purge volume control solenoid valve will be closed.

DTC No. | Trouble diagnosis name | DTC detecting condition | Possible cause
P0442 | EVAP control system small leak detected (negative pressure) | EVAP control system has a leak, EVAP control system does not operate properly. |

- Incorrect fuel tank vacuum relief valve
- Incorrect fuel filler cap used
- Fuel filler cap remains open or fails to close.
- Foreign matter caught in fuel filler cap.
- Leak is in line between intake manifold and EVAP canister purge volume control solenoid valve.
- Foreign matter caught in EVAP canister vent control valve.
- EVAP canister or fuel tank leaks
- EVAP purge line (pipe and rubber tube) leaks
- EVAP purge line rubber tube bent
- Loose or disconnected rubber tube
- EVAP canister vent control valve and the circuit
- EVAP canister purge volume control solenoid valve and the circuit
- Fuel tank temperature sensor
- O-ring of EVAP canister vent control valve is missing or damaged
- EVAP canister is saturated with water
- EVAP control system pressure sensor
- Fuel level sensor and the circuit
- Refueling EVAP vapor cut valve
- ORVR system leaks

■ CAUTION ■

- Use only a genuine NISSAN fuel filler cap as a replacement. If an incorrect fuel filler cap is used, the MIL may illuminate.
- If the fuel filler cap is not tightened properly, the MIL may illuminate.
- Use only a genuine NISSAN rubber tube as a replacement.

DTC CONFIRMATION PROCEDURE
1.PRECONDITIONING
If DTC Confirmation Procedure has been previously conducted, always perform the following procedure before conducting the next test.

1. Turn ignition switch OFF and wait at least 10 seconds.
2. Turn ignition switch ON.
3. Turn ignition switch OFF and wait at least 10 seconds.

TESTING CONDITION:

- Perform “DTC WORK SUPPORT” when the fuel level is between 1/4 and 3/4 full, and vehicle is placed on flat level surface.
- Always perform test at a temperature of 0 to 30°C (32 to 86°F).

NOTE：
Check that EVAP hoses are connected to EVAP canister purge volume control solenoid valve properly.
Do you have CONSULT-III?
YES>>GO TO 2.
NO>>GO TO 3.
2.PERFORM DTC CONFIRMATION PROCEDURE
With CONSULT-III

1. Turn ignition switch ON.
2. Turn ignition switch OFF and wait at least 10 seconds.
3. Turn ignition switch ON and select “DATA MONITOR” mode with CONSULT-III.
4. Check that the following conditions are met.COOLAN TEMP/S: 0 - 70°C (32 - 158°F)INT/A TEMP SE: 0 - 30°C (32 - 86°F)
5. Select “EVP V/S LEAK P0456/P1456” of “EVAPORATIVE SYSTEM” in “DTC WORK SUPPORT” mode with CONSULT-III.Follow the instructions displayed.
   NOTE：
   If the engine speed cannot be maintained within the range displayed on the CONSULT-III screen, go to Special Repair Requirement (GT-R certified NISSAN dealer).

Which is displayed on CONSULT-III screen?
OK>>INSPECTION END
NG>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
3.PERFORM DTC CONFIRMATION PROCEDURE
With GST
NOTE：
Be sure to read the explanation of SRT Set Driving Pattern (GT-R certified NISSAN dealer) before driving vehicle.

1. Start engine.
2. Drive vehicle according to SRT Set Driving Pattern (GT-R certified NISSAN dealer).
3. Turn ignition switch OFF and wait at least 10 seconds.
4. Turn ignition switch ON.
5. Turn ignition switch OFF, wait at least 10 seconds and then turn ON.
6. Check 1st trip DTC.

Is 1st trip DTC displayed?
YES-1>>P0441: Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
YES-2>>P0442: Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END