1.Set shock absorber horizontally with the piston rod fully extended.

2.Drill 2 – 3 mm (0.08 – 0.12 in) hole at the position () from top as shown in the figure to release gas gradually.
■ CAUTION ■

- Wear eye protection (safety glasses).
- Wear gloves.
- Be careful with metal chips or oil blown out by the compressed gas.

NOTE：

- Drill vertically in this direction ().
- Directly to the outer tube avoiding brackets.
- The gas is clear, colorless, odorless, and harmless.

A | : 20 – 30 mm (0.79 – 1.18 in)

3.Position the drilled hole downward and drain oil by moving the piston rod several times.
■ CAUTION ■
Dispose of drained oil according to the law and local regulations.