REMOVAL

1.Remove tires with power tool. Refer to Exploded View.

2.Remove under cover. Refer to Exploded View.

3.Remove stabilizer connecting rod.
■ CAUTION ■
Apply a matching mark to identify the installation position.

4.Remove stabilizer clamp and stabilizer bushing.

5.Remove stabilizer bar.

INSTALLATION
Note the following, and install in the reverse order of removal.

- Check the matching mark when installing.
- Never tap on the ball joint cap of the stabilizer connecting rod with a hammer or a similar item when inserting the stabilizer connecting rod into the transverse link.
- Tighten the mounting nut to the specified torque while holding a hexagonal part of stabilizer connecting rod side.