1.PERFORM COMPONENT FUNCTION CHECK With GST

1. Start engine and warm it up to normal operating temperature.
2. Drive the vehicle at a speed of 80 km/h (50 MPH) for a few minutes in the suitable gear position.
3. Shift the selector lever to A position, then release the accelerator pedal fully until the vehicle speed decreases to 50 km/h (31 MPH).
   ■ CAUTION ■
   Always drive vehicle at a safe speed.
   NOTE：
   Never apply brake during releasing the accelerator pedal.
4. Repeat steps 2 to 3 for five times.
5. Stop the vehicle and turn ignition switch OFF.
6. Wait at least 10 seconds.
7. Turn ignition switch ON.
8. Turn ignition switch OFF, wait at least 10 seconds and then restart engine.
9. Repeat steps 2 to 3 for five times.
10. Stop the vehicle.
11. Check 1st trip DTC.

Is 1st trip DTC detected?
YES>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END