1.SAVING VEHICLE SPECIFICATION CONSULT-III Configuration Perform “READ CONFIGURATION” to save or print current vehicle specification. Refer to Description. NOTE： If “READ CONFIGURATION” can not be used, use the “WRITE CONFIGURATION - Manual selection” after replacing BCM.
>>GO TO 2.
2.REPLACE BCM
Replace BCM. Refer to Exploded View.
>>GO TO 3.
3.WRITING VEHICLE SPECIFICATION
CONSULT-III Configuration
Perform “WRITE CONFIGURATION ‐ Config file” or “WRITE CONFIGURATION ‐ Manual selection” to write vehicle specification. Refer to Work Procedure.
>>GO TO 4.
4.INITIALIZE BCM (NATS)
Perform BCM initialization. (NATS)
>>WORK END