1.CHECK FRONT VERTICAL G SENSOR OUTPUT VOLTAGE

1. Connect the E-SUS control unit harness connector and front vertical G sensor harness connector.
2. Turn the ignition switch ON.
   ■ CAUTION ■
   Never start the engine.
3. Check the voltage between the E-SUS control unit harness connector and ground.

   E-SUS control unit | — | Voltage
   Connector | Terminal
   M110 | 4 | Ground | Approx. 2.35 – 2.65 V

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace the front vertical G sensor. Refer to Exploded View (GT-R certified NISSAN dealer).