1.CHECK TRUNK LID OPENER CANCEL SWITCH

1. Turn ignition switch OFF.
2. Disconnect trunk lid opener cancel switch connector.
3. Check continuity between trunk lid opener cancel switch terminals.

   Trunk lid opener cancel switch | Condition | Continuity
   Terminal
   1 | 2 | Trunk lid opener cancel switch | ON | Existed
   OFF (Cancel) | Not existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace trunk lid opener cancel switch. Refer to Removal and Installation.