DRIVE GEAR AND DRIVE PINION

- Wash the disassembled parts thoroughly.
- If the gear teeth are inadequate, investigate the cases and adjust to appropriate tooth contact.
- If the teeth are significantly worn, cracked, damaged, pitted, or chipped, replace transmission assembly.

BEARING

- Wash the disassembled parts thoroughly.
- If any chipped, pitted, worn, rusted, or scratched, or unusual noise is heard from the bearing, replace as a bearing assembly (as a new set) with new one.

SIDE BEARING ADJUSTING SHIM

- Wash the disassembled parts thoroughly.
- If the side bearing adjusting shim is chipped, damaged, or abnormally worn, replace the replace the side bearing adjusting shim.

OIL SEAL

- Whenever disassembled, replace.
- If the lip of oil seal is abnormally worn, deteriorated in tension (sealing force of lip), replace the oil seal with a new one.

DIFFERENTIAL CASE

- Wash the disassembled parts thraoughly.
- If the sliding part is worn or cracked, replace the differential case.