■ CAUTION ■ Be careful of the following items at removal and installation of A/T shift selector. Refer to Removal and Installation for details.

- For electro-medical apparatus user, keep the range sensor away from the device.
- Keep the range sensor away from magnetic objects during work.

REMOVAL
NOTE：
When replacing AV control unit, save or print current vehicle specification with CONSULT-III configuration before replacement. Refer to Special Repair Requirement.

1.Remove the cluster lid C (lower). Refer to Removal and Installation.

2.Disconnect the connector, and then remove the AV control unit together with the bracket from the vehicle.

3.Remove the bracket from the AV control unit.

INSTALLATION
Install in the reverse order of removal.
■ CAUTION ■
When replacing AV control unit, you must perform “WRITE CONFIGURATION” with CONSULT-III. Refer to Special Repair Requirement.