1.CHECK PASSENGER SIDE DOOR REQUEST SWITCH Check passenger side door request switch. Refer to Component Function Check. Is the inspection result normal? YES>>GO TO 2.
NO>>Repair or replace the malfunctioning parts.
2.CHECK OUTSIDE KEY ANTENNA RH
Check outside key antenna RH.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 3.
NO>>Repair or replace the malfunctioning parts.
3.CONFIRM THE OPERATION
Confirm the operation again.
Is the result normal?
YES>>Check Intermittent Incident. Refer to Intermittent Incident.
NO>>GO TO 1.