1.CHECK FRONT WIPER (AUTO STOP) SIGNAL CONSULT-III DATA MONITOR

1. Select “WIP AUTO STOP” of IPDM E/R data monitor item.
2. Operate the front wiper.
3. With the front wiper operation, check the monitor status.

   Monitor item | Condition | Monitor status
   WIP AUTO STOP | Front wiper motor | Stop position | STOP P
   Except stop position | ACT P

Is the status of item normal?
YES>>Auto stop signal circuit is normal.
NO>>Refer to Diagnosis Procedure.