1.CHECK SUB FUEL PUMP

1. Turn ignition switch OFF.
2. Disconnect ”fuel level sensor unit and fuel pump (sub fuel pump)” harness connector.
3. Check resistance between sub fuel pump terminals as follows.

   Terminals | Resistance
   1 and 2 | 0.2 - 0.5 Ω [at 25°C (77°F)]

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace “main fuel level sensor unit, fuel filter and fuel pump assembly”.