DTC DETECTION LOGIC

DTC | Display Item | Malfunction detected condition | Possible causes
C1755 | PR RECEIV COND FL | The data signal from the front LH wheel transmitter cannot be detected due to external electromagnetic interference. (DTC C1708 is displayed at the same time.) | External electromagnetic interference
C1756 | PR RECEIV COND FR | The data signal from the front RH wheel transmitter cannot be detected due to external electromagnetic interference. (DTC C1709 is displayed at the same time.)
C1757 | PR RECEIV COND RR | The data signal from the rear RH wheel transmitter cannot be detected due to external electromagnetic interference. (DTC C1710 is displayed at the same time.)
C1758 | PR RECEIV COND RL | The data signal from the rear LH wheel transmitter cannot be detected due to external electromagnetic interference. (DTC C1711 is displayed at the same time.)

■ CAUTION ■
If DTC C1755, C1756, C1757, or C1758 (low communication performance) is detected along with, C1708, C1709, C1710, or C1711 (no transmitter data) first diagnose C1755, C1756, C1757, or C1758 (low communications performance).
DTC REPRODUCTION PROCEDURE
1.DTC REPRODUCTION PROCEDURE
With CONSULT-III

1. Drive for 3 minutes at a speed of 40 km/h (25 MPH) or more, then drive normally for 10 minutes.
2. Perform self-diagnosis of the low tire pressure warning control unit.

Is DTC “C1755”, “C1756”, “C1757”, or “C1758 ” detected?
YES>>Perform trouble diagnosis. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END