Item | Function
BCM | Controls the door lock function.
IPDM E/R | Sounds horn and blinks headlamp via CAN communication with BCM.
Door lock actuator | Inputs lock/unlock signal from BCM and locks/unlocks each door.
Fuel lid lock actuator | Inputs lock/unlock signal from BCM and lock/unlocks fuel filler lid.
Door switch | Inputs door open/close condition to BCM.
Remote keyless entry receiver | Receives lock/unlock signal from the Intelligent Key, and then transmits to BCM.
Door request switch | Inputs lock/unlock operation to BCM.
Intelligent Key | Transmits button operation to remote keyless entry receiver.
Outside key antenna | Detects if Intelligent Key is outside the vehicle.
Inside key antenna | Detects if Intelligent Key is inside the vehicle.
Combination meter | Hazard warning lamp is installed to combination meter.
Push-button ignition switch | Inputs push-button ignition switch ON/OFF condition to BCM.
Intelligent Key warning buzzer | Warns the user of the lock/unlock condition and inappropriate operations with the buzzer sound.
Hazard warning lamp | Warns the user of the door lock/unlock condition and in appropriate operations with the lamps blink.