- There are 2 different power supply systems for the range sensors; the range sensor power supply 1 system distributes power supply to 4 range sensors (No. 0, No. 1, No. 3, and No. 5) used for the range position recognition, and the auto/manual range change switch changing between M range and A range. The range sensor power supply 2 system distributes power supply to 2 range sensors (No. 2 and No. 4) used for the range position recognition.
- TCM recognizes the shift lever position by combining signals from 6 range sensors used for the range position recognition and park position switch.

TCM recognized position | Shift lever position | Park position switch | Range sensor
No. 0 | No. 1 | No. 2 | No. 3 | No. 4 | No. 5
P | P | ON | ON | OFF | OFF | OFF | OFF | OFF
R | R | OFF | OFF | ON | ON | OFF | OFF | OFF
N | N | OFF | OFF | OFF | ON | ON | ON | OFF
A/M | A/M | OFF | OFF | OFF | OFF | OFF | ON | ON