1.CHECK AIR BAG MODULE Check the deployment of front air bag module. Is air bag module deployed? YES>>Refer to the following items. Exploded View (Driver air bag module) Exploded View (Front passenger air bag module) Exploded View (Front side air bag module) Exploded View (Side curtain air bag module).
NO>>GO TO 2.
2.CHECK AIR BAG FUSE
Check the air bag fuse. Refer to Fuse.
Is 10A fuse [No.2, located in fuse block (J/B)] normal?
YES>>GO TO 4.
NO>>Replace the air bag fuse and GO TO 3.
3.CHECK AIR BAG FUSE AGAIN
Turn ignition switch ON.
Check the air bag fuse. Refer to Fuse.
Does the air bag fuse blow again?
YES>>Repair or replace related harness.
NO>>GO TO 4.
4.CHECK SELF DIAGNOSIS RESULT
Perform “AIR BAG” Self Diagnostic result.
Is DTC detected?
YES>>Repair or replace the malfunctioning parts.
NO>>Check the intermittent incident. Refer to Intermittent Incident.