INSPECTION AFTER INSTALLATION

1.Check the brake hoses and tubes for the following: no scratches; no twist and deformation; no interference with other components when turning the steering wheel; no looseness at connections.

2.Depress the brake pedal with a force of 785 N (80 kg, 177 lb) and hold down the pedal for approximately 5 seconds with the engine running. Check for any fluid leakage.
■ CAUTION ■
Retighten the applicable connection to the specified torque and repair any malfunctioning (damaged, worn or deformed) parts if any brake fluid leakage is present.