REMOVAL

1.Operate the front wiper to move it to the auto stop position.

2.Open the hood.

3.Remove the front wiper arm caps.

4.Remove the front wiper arm mounting nuts.

5.Disconnect the front washer tube from the front washer joint.

6.Raise front wiper arm, and remove front wiper arm from the vehicle.

INSTALLATION

1.Clean wiper arm mount as shown in the figure to prevent nuts from being loosened.

2.Operate the front wiper motor to move the front wiper to the auto stop position.

3.Adjust the front wiper blade position. Refer to Adjustment.

4.Install the front wiper arm by tightening the mounting nuts.

5.Connect the front washer tube to the front washer joint.

6.Inject the washer fluid.

7.Operate the front wiper to move it to the auto stop position.

8.Check that the front wiper blades stop at the specified position.

9.Install the front wiper arm caps.