REMOVAL

1.Remove radiator. Refer to Exploded View (GT-R certified NISSAN dealer).

2.Disconnect harness connector from cooling fan control module, and move harness to aside.

3.Remove cooling fan control module.
■ CAUTION ■
Handle carefully to avoid dropping and shocks.

4.Remove cooling fan mounting nuts, and then remove the cooling fans (RH and LH).

5.Remove fan motors (RH and LH).

- Identify installation positions, and store them without mixing them up.

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■
RH and LH fan motors are different. Be careful not to misassemble them.

- Install each fan in the following position.
  ■ CAUTION ■
  RH and LH cooling fans are different. Be careful not to misassemble them.

  Right side | : 9 blades
  Left side | : 7 blades

- Apply high strength thread locking sealant on fan motor shaft.

- Secure the harness tightly to the fan shroud to prevent the fan rotation area from being loose.