Component | Function
BCM |

- Supplies the power to power window main switch and power window sub-switch
- Supplies power to driver side and passenger side power window motor
- Controls retained power

Power window main switch |

- Outputs the UP or DOWN signal to driver side and passenger side power window motor
- Power window lock switch is equipped, and when the button is pressed (LOCK), deactivates the assistant seat power window operation

Power window sub-switch | Outputs the UP or DOWN signal to passenger side power window motor
Driver side power window motor |

- Operates by UP or DOWN signal from power window main switch
- Encoder: Detects power window motor speed by 2 pulse signals
- Module: Controls the anti-pitch, Auto operation, and automatic window adjusting functions by the pulse signal from encoder

Passenger side power window motor |

- Operates by UP or DOWN signal from power window main switch or assistant seat power window switch
- Encoder: Detects power window motor speed by 2 pulse signals
- Module: Controls the anti-pitch and automatic window adjusting functions by the pulse signal from encoder

Door switch | Detects the driver side and passenger side doors open or closed condition