- Replace the propeller shaft assembly if there is a breakage or deflection on the tube.
- Never hit the tube or apply an impact on it during repair service. Never damage the tube as well.
- The joint cannot be disassembled. Never disassemble it.
- If a constant velocity universal joint is bent during removal, installation, or transportation of the propeller shaft assembly, the joint may be damaged. Wrap a shop cloth or rubber sheet around the joint to protect it from being damaged.
- The main propeller shaft is constantly rotating while the engine is running. To prevent interference, stop the engine before removing or installing the propeller shaft assembly.