DTC DETECTION LOGIC NOTE： If DTC B2110 is displayed with DTC U1000, first perform the trouble diagnosis for DTC U1000. Refer to DTC Logic.

DTC No. | Trouble diagnosis name | DTC detecting condition | Possible cause
B2110 | INTER LOCK/PNP SW | IPDM E/R detects the difference between the signals below for 1 second or more.

- P/N position signal from TCM
- Shift position signal from BCM (CAN)

- Harness or connectors
  (TCM circuit is open or shorted)
- TCM
- IPDM E/R
- BCM

DTC CONFIRMATION PROCEDURE
1.PERFORM DTC CONFIRMATION PROCEDURE

1. Turn the ignition switch ON under the following conditions and wait for at least 1 second.

- Shift lever is in the P or N position.
- Do not depress brake pedal.

2. Check “Self diagnostic result” with CONSULT-III.

Is DTC detected?
YES>>Go to Diagnosis Procedure.
NO>>INSPECTION END