Vehicle specification needs to be written with CONSULT‐III because it is not written after replacing BCM. Configuration has three functions as follows.

Function | Description
READ CONFIGURATION |

- Reads the vehicle configuration of current BCM.
- Saves the read vehicle configuration.

WRITE CONFIGURATION - Manual selection | Writes the vehicle configuration with manual selection.
WRITE CONFIGURATION - Config file | Writes the vehicle configuration with saved data.
NOTE：
Manual setting item: Items which need selection by vehicle specifications
Automatic setting item: Items which are written in automatically (Setting can not be changed)

■ CAUTION ■

- When replacing BCM, you must perform “WRITE CONFIGURATION” with CONSULT‐III.
- Complete the procedure of “WRITE CONFIGURATION” in order.
- If you set incorrect “WRITE CONFIGURATION”, incidents might occur.
- Configuration is different for each vehicle model. Confirm configuration of each vehicle model.
- Never perform “WRITE CONFIGURATION” except for new BCM.