REMOVAL ■ CAUTION ■ Disconnect the battery negative terminal or remove the fuse.

1.Remove front bumper fascia. Refer to Exploded View.

2.Remove the headlamp mounting bolts.

3.Remove the harness clip (A) and the washer tube (B)*.*: Left side only

4.Pull out the headlamp assembly forward the vehicle.

5.Disconnect the connector before removing the headlamp housing assembly.

INSTALLATION
Install in the reverse order of removal.
■ CAUTION ■

- After installation, perform aiming adjustment. Refer to Description.
- After installation, check that headlamp lighting. Refer to Inspection After Installation (HID Control Unit).
- When the front combination lamp on one side is replaced, and rubber seal is not installed to the front combination lamp on the side that is not replaced, install a rubber seal to the front combination lamp that is not replaced as per the following procedure.
- Always clean the front combination lamp surface where rubber seal is affixed.

1.Align rubber seal (1) with lens inner protrusion (A) and affix so that there is not gap.

2.Align rubber seal edge (1) with hood seal assembly edge (2) and affix under hood seal assembly.

3.Align rubber seal end (1) with hood end (3) and affix so that it does not protrude from hood.