REMOVAL

1.Remove tires with power tool. Refer to Exploded View.

2.Remove shock absorber from axle housing with power tool.

3.Remove rear parcel shelf finisher. Refer to Exploded View.

4.Remove shock absorber actuator harness connector (A) and seat (1).

| : Vehicle front

5.Remove shock absorber assembly.

INSTALLATION
Note the following, and install in the reverse order of removal.

- Install the seat to cover the shock absorber actuator harness connector.
- Perform final tightening of bolts and nuts at the vehicle installation position (rubber bushing), under unladen conditions with tires on level ground.