The actual shapes of Kent‐Moore tools may differ from those of special service tools illustrated here. HFC-134a (R-134a) Service Tool and Equipment

- Never mix HFC‐134a (R‐134a) refrigerant and/or its specified lubricant with CFC‐12 (R‐12) refrigerant and/or its lubricant.
- Separate and non‐interchangeable service equipment must be used for handling each type of refrigerant/lubricant.
- Refrigerant container fittings, service hose fittings and service equipment fittings (equipment which handles refrigerant and/or lubricant) are different between CFC‐12 (R‐12) and HFC‐134a (R‐134a). This is to avoid mixed use of the refrigerants/lubricant.
- Never use adapters that convert one size fitting to another: refrigerant/lubricant contamination occurs and compressor malfunction may result.

Tool number (Kent‐Moore No.) Tool name | Description
(J‐45815) Disconnector tool set |  | Disconnect one‐touch joint connection
(ACR2005‐NI) ACR5 A/C Service Center |  | Function: Refrigerant recovery, recycling and recharging
(J‐41995) Electrical leak detector |  | Power supply: DC 12 V (Battery terminal)
(J‐43926) Refrigerant dye leak detection kit Kit includes: (J‐42220) UV lamp and UV safety goggles
(J‐41459)
HFC‐134a (R‐134a) dye injector
Use with J‐41447, 1/4 ounce bottle
(J‐41447)
HFC‐134a (R‐134a) fluorescent leak detection dye
(Box of 24, 1/4 ounce bottles)
(J‐43872)
Refrigerant dye cleaner
Power supply:
DC 12 V (Battery terminal)
(J‐42220) UV lamp and UV safety goggles |  | Power supply: DC 12 V (Battery terminal) For checking refrigerant leakage when fluorescent dye is equipped in A/C system Includes: UV lamp and UV safety goggles
(J‐41447) HFC‐134a (R‐134a) fluorescent leak detection dye (Box of 24, 1/4 ounce bottles) |  | Application: For HFC‐134a (R‐134a) PAG oil Container: 1/4 ounce (7.4 cc) bottle (Includes self‐adhesive dye identification labels for affixing to vehicle after charging system with dye.)
(J‐41459) HFC‐134a (R‐134a) dye injector Use with J‐41447, 1/4 ounce bottle |  | For injecting 1/4 ounce of fluorescent leak detection dye into A/C system
(J‐43872) Refrigerant dye cleaner |  | For cleaning dye spills
(J‐39183) Manifold gauge set (with hoses and couplers) |  | Identification:

- The gauge face indicates HFC‐134a (R‐134a).

Fitting size: Thread size

- 1/2″‐16 ACME

Service hoses

- High‐pressure side hose
  (J‐39501‐72)
- Low‐pressure side hose
  (J‐39502‐72)
- Utility hose
  (J‐39476‐72)

Hose color:

- Low‐pressure side hose: Blue with black stripe
- High‐pressure side hose: Red with black stripe
- Utility hose: Yellow with black stripe or green with black stripe

Hose fitting to gauge:

- 1/2″‐16 ACME

Service couplers

- High‐pressure side coupler
  (J‐39500‐20)
- Low‐pressure side coupler
  (J‐39500‐24)

Hose fitting to service hose:
M14 x 1.5 fitting is optional or permanently attached.
(J‐39650) Refrigerant weight scale |  | For measuring of refrigerant Fitting size: Thread size 1/2″‐16 ACME
(J‐39649) Vacuum pump (Including the isolator valve) |  | Capacity:

- Air displacement: 4 CFM
- Micron rating: 20 microns
- Oil capacity: 482 g (17 oz.)

Fitting size: Thread size

- 1/2″‐16 ACME