■ CAUTION ■ Due to varying models and option levels, not all parts listed in the chart below apply to all vehicles. WORK PROCEDURE

1.Before performing any of the following steps, ensure that all vehicle body and structural repairs have been completed.

2.Replace the following components:

- Front seat back assembly (on the side on which side air bag is activated)
- Door finisher (on the side on which door-mounted curtain air bag is activated)
- Pop-up roll bar assemblies and pop-up roll bar covers
- Side air bag (satellite) sensor LH/RH (on the side on which side air bag is activated)
- Diagnosis sensor unit
- Seat belt pre-tensioner assemblies

3.Check the SRS components and the related parts using the following table.Replace any SRS components and the related parts showing visible signs of damage. (dents, cracks, deformation, etc.)

4.Perform self-diagnosis using CONSULT-III and “AIR BAG” warning lamp. Refer to CONSULT-III Function or Air Bag Warning Lamp Diagnosis for details. Make sure entire SRS operates properly.

5.After the work is completed, perform self-diagnosis to check that no malfunction is detected. Refer to Diagnosis Description.

SRS INSPECTION (FOR SIDE AND ROLLOVER COLLISION)

Part | Inspection
Side curtain air bag module LH | If the side curtain air bag LH has deployed: REPLACE the side curtain air bag module LH. Install with new fasteners.
Side curtain air bag module RH | If the side curtain air bag RH has deployed: REPLACE the side curtain air bag module RH. Install with new fasteners.
Front side air bag module LH | If the front side air bag LH has deployed: REPLACE front seatback assembly LH.
Front side air bag module RH | If the front side air bag RH has deployed: REPLACE front seatback assembly RH.
Side air bag (satellite) sensor (LH or RH) | If any of the SRS components have deployed: REPLACE the side air bag (satellite) sensor on the collision side with new fasteners.
Diagnosis sensor unit | If any of the SRS components have deployed: REPLACE the diagnosis sensor unit with new fasteners.
Seat belt pre-tensioner assemblies (All applicable locations: buckle, retractor, lap outer) | If either the driver or passenger seat belt pre-tensioner* has been activated: REPLACE all seat belt pre-tensioner assemblies with new fasteners. *: Confirm seat belt pre-tensioner activation using CONSULT-III only.
Center inner pillar |

1. Check the center inner pillar on the collision side for damage (dents, cracks, deformation, etc.).
2. If damaged − REPAIR the center inner pillar.

Trim/headlining |

1. Check for visible signs of damage (dents, cracks, deformation, etc.) of the interior trim on the collision side.
2. If damaged − REPLACE the damaged trim parts.

Door-mounted curtain air bag module LH | If the door-mounted curtain air bag module LH has deployed: REPLACE the door finisher LH and door-mounted curtain air bag module. Install with new fasteners.
Door-mounted curtain air bag module RH | If the door-mounted curtain air bag module RH has deployed: REPLACE the door finisher RH and door-mounted curtain air bag module. Install with new fasteners.
Pop-up roll bar assemblies | If the pop-up roll bar has deployed: REPLACE pop-up roll bar assemblies and pop-up roll bar covers. Install with new fasteners.