1.ECM SELF-DIAGNOSIS Perform self-diagnosis for “ENGINE” with CONSULT-III. Is any DTC detected? YES>>Check the DTC. NO>>GO TO 2.
2.ABS ACTUATOR AND ELECTRIC UNIT (CONTROL UNIT) SELF-DIAGNOSIS

1. Erase self-diagnosis results for “ABS” with CONSULT-III.
2. Turn the ignition switch OFF.
3. Start the engine. Drive the vehicle for a while.
4. Check that malfunction indicator lamp (MIL) turns OFF.
5. Stop the engine. Perform self-diagnosis for “ABS” with CONSULT-III.

Is DTC “C1130” detected?
YES>>Replace ABS actuator and electric unit (control unit). Refer to Exploded View (GT-R certified NISSAN dealer).
NO>>Check ABS actuator and electric unit (control unit) pin terminals for damage or loose connection with harness connector. If any items are damaged, repair or replace error-detected parts.