■ CAUTION ■ Wrap the tip of flat-bladed screwdriver with a shop cloth before remove. REMOVAL

1.Fully open the door window.

2.Insert a remover tool (A) into the lower side of door grip cap (1), then disengage and remove the pawls and metal clips.

| : Pawl
| : Metal clip

3.Insert a remover tool (A) between the door finisher and rear of armrest (1), disengage the pawls and metal clips and then remove the armrest.

| : Pawl
| : Metal clip

4.Remove the door finisher tightening bolts (A) shown in the figure.

5.Remove the clip from the door finisher rear end. Refer to Exploded View.

6.Disengage the clips from the door finisher (1) rear side using a remover tool (A).
■ CAUTION ■
Insert the remover tool between door panel and clip, and then disengage the clip.

| : Clip

7.Remove the door finisher rear side lock knob cable (2) and the inside handle cable (1) from the inside handle (A).

8.Lift up the door finisher and pull it out toward the passenger room. Disconnect the connectors (A) and (B) from the door finisher rear side.

9.Remove the door finisher.

10.Remove the front door squawker (BOSE AUDIO WITH NAVIGATION) after removing the door finisher. Refer to Removal and Installation.

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■
When installing the door finisher, check that the clips are securely fitted in panel holes, and then press them in.