The actual shapes of Kent-Moore tools may differ from those of special service tools illustrated here.
Tool number (Kent-Moore No.) Tool name |  | Description
KV40101000 (　　—　　) Attachment |  | Removing side flange
ST36230000 (J-25840-A) Sliding hammer |  | Removing side flange
KV40104830 (　　—　　) Drift a: 70 mm (2.76 in) dia. b: 63.5 mm (2.50 in) dia.
Installing side oil seal
KV38105500 (J-33904) Protector a: 40 mm (1.57 in) dia. |  | Installing side flange
ST33081000 (　　—　　) Drift a: 43 mm (1.69 in) dia. b: 33.5 mm (1.319 in) dia.
Removing side bearing inner race
KV40104730 (　　—　　) Drift a: 53.7 mm (2.114 in) dia. |  | Installing side bearing inner race
KV40104720 (　　—　　) Adapter a: 76 mm (2.99 in) dia. b: 64 mm (2.52 in) dia.
c: 56 mm (2.20 in) dia.
d: 67.5 mm (2.657 in) dia.
e: 63.7 mm (2.508 in) dia.
f: 48 mm (1.89 in) dia.
Installing side bearing inner race
KV10112100 (BT‐8653‐A) Angle wrench |  | Tightening the drive gear mounting bolt
ST01500001 (　　—　　) Drift a: 89 mm (3.50 in) dia. b: 79 mm (3.11 in) dia.
Installing side bearing outer race
KV40105310 (　　—　　) Drift a: 89.1 mm (3.508 in) dia. b: 80.7 mm (3.177 in) dia.
Installing side bearing outer race (side cover side)
KV40104710 (　　—　　) Drift a: 76.3 mm (3.004 in) dia. b: 67.9 mm (2.673 in) dia.
Installing side bearing outer race (gear carrier side)