1.PERFORM THE DECEL G SENSOR CALIBRATION Perform the decel G sensor calibration. Refer to Special Repair Requirement (GT-R certified NISSAN dealer). Is calibration of decel G sensor finished? YES>>INSPECTION END NO>>GO TO 2.
2.CHECK YAW RATE/SIDE/DECEL G SENSOR
Check yaw rate/side/decel G sensor. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
Is the inspection result normal?
YES>>Replace ABS actuator and electric unit (control unit). Refer to Exploded View (GT-R certified NISSAN dealer).
NO>>Repair or replace error-detected parts.