1.CHECK FUEL PRESSURE-I Check fuel pressure. (Refer to Inspection (GT-R certified NISSAN dealer)) Is the inspection result normal? YES>>GO TO 2. NO>>Repair or replace.
2.CHECK FUEL PRESSURE-II

1. Start engine.
2. Select “SUB FUEL PUMP RELAY” in “ACTIVE TEST” mode with CONSULT-III.
3. Touch “ON”.
4. Read the indication of fuel pressure gauge.

   At idling | : Approximately 350 kPa (3.57 kg/cm2, 51 psi)

Is the inspection result normal?
YES>>GO TO 3.
NO>>Replace “main fuel level sensor unit, fuel filter and fuel pump assembly”.
3.CHECK INTERMITTENT INCIDENT
Refer to Intermittent Incident.
>>INSPECTION END