OVERALL SEQUENCE DETAILED FLOW 1.OBTAIN INFORMATION ABOUT SYMPTOM Interview the customer to obtain as much information as possible about the conditions and environment under which the malfunction occurred. >>GO TO 2.
2.CHECK SYMPTOM

- Check the symptom based on the information obtained from the customer.
- Check if any other malfunctions are present.

>> GO TO 3.
3.CHECK CONSULT‐III SELF-DIAGNOSIS RESULTS
Connect CONSULT‐III and perform self-diagnosis. Refer to CONSULT-III Function (METER/M&A).
Are self-diagnosis results normal?
YES>>GO TO 4.
NO>>GO TO 5.
4.NARROW DOWN MALFUNCTIONING PARTS BY SYMPTOM DIAGNOSIS
Perform symptom diagnosis and narrow down the malfunctioning parts.
>>GO TO 5.
5.REPAIR OR REPLACE MALFUNCTIONING PARTS
Repair or replace malfunctioning parts.
NOTE：
If DTC is displayed, erase DTC after repairing or replacing malfunctioning parts.
>>GO TO 6.
6.FINAL CHECK
Check that the warning buzzer in the combination meter operates normally.
Does it operate normally?
YES>>INSPECTION END
NO>>GO TO 1.