TERMINAL LAYOUT PHYSICAL VALUES

Terminal (Wire color) | Description | Condition | Reference value (Approx.)
+ | – | Signal name | Input/Output
6 | — | Shield | — | — | — | —
9 (SB) | Ground | Communication signal (DISP→CONT) | Output | Ignition switch ON | When adjusting display brightness. |
10 (V) | Ground | Communication signal (CONT→DISP) | Input | Ignition switch ON | When adjusting display brightness. |
11 (Y) | Ground | Battery power supply | Input | Ignition switch OFF | — | Battery voltage
12 (B) | Ground | Ground | — | Ignition switch ON | — | 0 V
18 (R) | Ground | Composite image signal | Input | Ignition switch ON | At DVD image is displayed. |
19 (W) | Ground | Composite image ground | — | Ignition switch ON | — | 0 V
20 (B) | Ground | Composite synchronizing signal | Input | Ignition switch ON | — |
22 | — | Shield | — | — | — | —
23 (P) | Ground | ACC power supply | Input | Ignition switch ACC | — | Battery voltage
27 | — | RGB digital image signal (+) | Input | — | — | —
28 | — | RGB digital image signal (−) | Input | — | — | —