Tool name (Kent-Moore No.) |  | Description
Leak detector i.e.: (J-41416) |  | Locates the EVAP leak
EVAP service port adapter i.e.: (J-41413-OBD) |  | Applys positive pressure through EVAP service port
Fuel filler cap adapter i.e.: (MLR-8382) |  | Checks fuel tank vacuum relief valve opening pressure
Socket wrench |  | Removes and installs engine coolant temperature sensor
Oxygen sensor thread cleaner i.e.: (J-43897-18) (J-43897-12) |  | Reconditions the exhaust system threads before installing a new oxygen sensor. Use with anti-seize lubricant shown below. a: 18 mm diameter with pitch 1.5 mm for Zirconia Oxygen Sensor b: 12 mm diameter with pitch 1.25 mm for Titania Oxygen Sensor
Anti-seize lubricant i.e.: (PermatexTM 133AR or equivalent meeting MIL specification MIL-A-907) |  | Lubricates oxygen sensor thread cleaning tool when reconditioning exhaust system threads.