CONTROL OUTLINE The combination meter reads the fuel level sensor signal (resistance value) from the fuel level sensor unit, and indicates the fuel level to the fuel gauge. REFUEL CONTROL When the ignition switch is turned from OFF to ON, or when all the following conditions are met, it performs a control to move the fuel gauge pointer faster than normal.

- Ignition switch ON
- Vehicle stop status
- Fuel level fluctuation is 15 (4 US gal, 3-1/4 lmp gal) or more.