NOTE： Details of time display

- CRNT: Displays during the current malfunctioning detection.
- PAST: Displays if any previous malfunction is present when the current status is normal.

IGN counter

- The IGN counter is displayed in the freeze frame data (FFD).
- The IGN counter indicates the number of times ignition switch is turned ON after the DTC detection.

- When a trouble is currently being detected, it displays “0”.
- After the status returns to normal, the indication value is incriminated as “1 → 2 → 3 → ... 38 → 39" every time the ignition switch is turned OFF → ON.
- When the operation count of ignition switch OFF → ON exceeds 39, the indication will be fixed at "39" until the self-diagnosis is deleted.

Display contents of CONSULT‐III | Diagnostic item is detected if ... | Refer to
CAN COMM CIRCUIT [U1000] | Combination meter cannot communicate CAN communication signal for 2 seconds or more | Diagnosis Procedure
CONTROL UNIT (CAN) [U1010] | Malfunction is detected during initial diagnosis of combination meter CAN controller | Diagnosis Procedure
VEHICLE SPEED [B2205] | Abnormal vehicle speed signal is received from ABS actuator and electric unit (control unit) for 2 seconds or more | Diagnosis Procedure
ENGINE SPEED [B2267] | ECM continuously transmits abnormal engine speed signal for 2 seconds or more | Diagnosis Procedure
WATER TEMP [B2268] | ECM continuously transmits abnormal coolant temperature signal for 60 seconds or more | Diagnosis Procedure
OIL LEV SEN OPEN [B2321] | Signal from oil level sensor is open (resistance value of oil level sensor is larger than 20 Ω). | Diagnosis Procedure
OIL LEV SEN SHORT [B2322] | Signal from oil level sensor is shorted (resistance value of oil level sensor is smaller than 3 Ω). | Diagnosis Procedure