REMOVAL

1.Remove dash side lower finisher (RH) and kicking plate inner (RH). Refer to Exploded View.

2.Remove front seat (passenger side). Refer to Removal and Installation.

3.Remove front seat belt (passenger side) outer anchor mounting anchor belt. Refer to Exploded View.

4.Turn over the floor trim of passenger seat side. Refer to Removal and Installation.

5.Remove the tool-box.

6.Remove the mounting bolts, and then remove the trunk lid key cylinder.

7.Disengage the joint of trunk lid lock control cable from the trunk lid key cylinder.

8.Remove the rear seat cushion (LH/RH) and the rear seatback (LH/RH). Refer to Removal and Installation.

9.Remove rear seat center finisher. Refer to Exploded View.

10.Remove the rear side finisher (RH). Refer to Exploded View.

11.Disengage the clip connecting the trunk lid lock control cable of passenger room side with the vehicle body.

12.Remove the trunk front finisher, trunk rear finisher, trunk side finisher back (LH), trunk side finisher upper (LH), and trunk side finisher lower (LH). Refer to Removal and Installation.

13.Disengage the clip connecting the trunk lid lock control cable of trunk room side with the vehicle body.

14.Remove the trunk lid striker. Refer to Removal and Installation.

15.Disengage the joint of trunk lid lock control cable from the trunk lid striker.

16.Pull out the trunk lid control cable toward passenger room side or trunk room side to remove.

INSTALLATION
Install in the reverse order of removal.
■ CAUTION ■

- After installation, check trunk lid open/close, lock/unlock operation.
- After installation, perform the fitting adjustment. Refer to Adjustment.