DTC DETECTION LOGIC

DTC | Self-diagnosis name | DTC detection condition | Possible cause
P0711 | Transmission fluid temperature sensor "A" circuit range/performance |

- A DTC is set if TCM detects the fluid temperature sensor value of 160°C (320°F) or more for a certain period of time.
- A DTC is set if TCM detects the fluid temperature sensor value of 0°C (32°F) or more and less than 20°C (68°F) for a certain period of time.
- A DTC is set if TCM detects the fluid temperature sensor value of −20°C (−4°F) or more, or less than 0°C (32°F) for a certain period of time.
- A DTC is set if TCM detects the fluid temperature sensor value of less than −20°C (−4°F) for a certain period of time.

- Fluid temperature sensor
- Harness or connector
  (Open or shorted in the fluid temperature sensor circuit)

DTC CONFIRMATION PROCEDURE
1.PREPARATION BEFORE OPERATION
If another “DTC CONFIRMATION PROCEDURE” is performed just before the next test, turn the ignition switch OFF and wait for 10 seconds or more, then perform the next test.
>>GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDURE
With CONSULT-III

1. Start the engine and run at idle for 8 minutes or more.
2. Check “Self Diagnostic Result” of “TRANSMISSION”.

Without CONSULT-III

1. Start the engine and run at idle for 8 minutes or more.
2. Check self-diagnosis.

Is DTC P0711 detected?
YES>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>Go to Intermittent Incident.