REMOVAL

1.Remove tires with power tool. Refer to Exploded View.

2.Remove under cover. Refer to Exploded View.

3.Remove steering knuckle. Refer to Exploded View.

4.Separate shock absorber form transverse link with power tool. Refer to Exploded View.

5.Set suitable jack under front suspension member.

6.Loosen front suspension member mounting bolts and nuts, and gradually lower jack to front suspension member. Refer to Exploded View.
■ CAUTION ■
Never remove front suspension member mounting bolts and nuts.

7.Remove transverse link.

INSTALLATION
Note the following, and install in the reverse order of removal.

- Perform final tightening of bolts and nuts at the vehicle installation position (rubber bushing), under unladen conditions with tires on level ground.
- Never reuse cotter pin.