DTC DETECTION LOGIC

DTC | Display item | Malfunction detected condition | Possible cause
C1101 | RR RH SENSOR-1 | Circuit of rear RH wheel sensor is open or shorted. Or when the sensor power voltage is outside the standard. |

- Harness or connector
- Wheel sensor
- ABS actuator and electric unit (control unit)

C1102 | RR LH SENSOR-1 | Circuit of rear LH wheel sensor is open or shorted. Or when the sensor power voltage is outside the standard.
C1103 | FR RH SENSOR-1 | Circuit of front RH wheel sensor is open or shorted. Or when the sensor power voltage is outside the standard.
C1104 | FR LH SENSOR-1 | Circuit of front LH wheel sensor is open or shorted. Or when the sensor power voltage is outside the standard.

DTC CONFIRMATION PROCEDURE
1.DTC REPRODUCTION PROCEDURE

1. Start the engine and drive the vehicle at 30 km/h (19 MPH) or more for approximately 1 minute.
2. Perform self-diagnosis for “ABS” with CONSULT-III.

Is DTC “C1101”, “C1102”, “C1103” or “C1104” detected?
YES>>Proceed to diagnosis. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END