RADIATOR CORE SUPPORT ASSEMBLY Disassembly

1.Remove the crash zone sensor. Refer to Removal and Installation.

2.Remove the cooling fan (LH/RH), cooling fan control module, fan motor, and fan motor cover. Refer to Removal and Installation (GT-R certified NISSAN dealer).

3.Remove all flaps.

Assembly
Assemble in the reverse order of disassembly.
AIR INTAKE DUCT ASSEMBLY
Disassembly

1.Remove the rivets, and then remove the air intake duct assembly 2.
NOTE：
Removal and installation of rivet

- Grind the head of rivet (1) with a drill (A) (blade of φ4.0 - 4.5 mm), and then remove the air intake duct 2.
- Securely crimp it with the air intake duct 2 using a hand riveter (B).

Air intake duct
Crimping thickness | : 0.5 – 6.4 mm (0.020 – 0.252 in)
Prepared hole diameter | : φ 5.1

2.Remove the charge air cooler. Refer to Removal and Installation.

3.Remove the mounting bolts, and then remove the bumper fascia bracket.

4.Remove the horn (HIGH/LOW). Refer to Removal and Installation.

5.Remove the ambient sensor. Refer to Removal and Installation.

6.Remove the clips and mounting bolts, and then remove the air guide bracket.

Assembly
Assemble in the reverse order of disassembly.